
*Note –To install WinCMM 3.0.8, you must install each version in the following sequence: version 2.0.0, version 2.0.2, and version 3.0.8. The following instructions detail the WinCMM 3.0.8 installation process.*

1. Install WinCMM version 2.0.0.
   1. Log on an account with administrator privileges.
   2. In the **CMM\_200** folder, double-click **Setup.exe**.
   3. When prompted, click **Yes** to retain the Microsoft HTML Help Executable (C:\Windows\System32\hh.exe).




* 1. When prompted, click **Yes** to retain the Microsoft InfoTech IR Local DLL  
     (C:\Windows\System32\itircl.dll).
  2. When prompted, click **Yes** to retain the Microsoft InfoTech Storage System Library(C:\Windows\System32\itss.dll).
  3. When prompted, click **Yes** to retain the Microsoft HTML Help Control(C:\Windows\System32\HHCTRL.ocx).
  4. When prompted, click **Yes** to retain the OLE 2.1 16/32 Interoperability Library(C:\Windows\System32\TYPELIB.DLL).
  5. When prompted, click **Yes** to retain the OLE 2.1 16/32 Interoperability Library(C:\Windows\System32\OLE2NLS.DLL).
  6. When prompted, click **Yes** to retain the OLE 2.1 16/32 Interoperability Library(C:\Windows\System32\OLE2DISP.DLL).
  7. When prompted, click **Yes** to retain the Microsoft C Runtime Library(C:\Windows\System32\MSVCRT20.DLL).


1. Apply the WinCMM 2.0.2 patch.
   1. On the computer, navigate to the WinCMM directory. (The default location is C:\Program Files (x86)\Cadastral Measurement Management.)
   2. Using the **winCMM.exe** file in the **CMM\_202** installation folder, overwrite the current version of **winCMM.exe** file in the WinCMM directory.
      1. In the installation folder, copy the **winCMM.exe** file.
      2. In the WinCMM directory, paste the **winCMM.exe** file.

*Note – A drag-and-drop action cannot be used to complete this task.*


* + 1. When prompted, click **Copy and Replace** to overwrite the file.



* + 1. When prompted for administrator permissions to copy to the destination folder, click **Continue**.




* + 1. When prompted to allow the program to make changes to the computer, click **Yes**.




1. Apply the WinCMM 3.0.8 patch.
   1. On the computer, navigate to the WinCMM directory. (The default location is C:\Program Files (x86)\Cadastral Measurement Management.)
   2. Using the corresponding filesin the **CMM\_308** installation folder, overwrite the current version of the following files:


* Blunder.exe
* Combin.exe
* Compar.exe
* Convert.exe
* Curvey.exe
* Raw.exe
* Sortsla.exe
* Tds.exe
* Utm.exe
* Whatis.exe
  + 1. In the **CMM\_308** installation folder, copy each of the files.
    2. In the **Cadastral Measurement Management** folder, paste each of the copied files.  
       *Note – A drag-and-drop action cannot be used to complete this task.*
    3. When prompted, select the **Do this for the next 9 conflicts** check box.
    4. Click **Copy and Replace** to overwrite the files.



* + 1. When prompted for administrator permissions to copy to the destination folder, click **Continue**.



* + 1. When prompted to allow the program to make changes to the computer, click **Yes**.



You have successfully completed the installation of WinCMM 3.0.8

1. To confirm the installation, open the **WinCMM** directory using the **Start** menu.
   1. Click **Start**.
   2. Click **All Programs**.
   3. Click **Cadastral Measurement Management**.
   4. Click **WinCMM**.